[국문초록예시]

Phase transformation of precipitates in steels

허윤욱

포항공과대학교 철강대학원

E-mail: yunuk01@postech.ac.kr

철강재료는 기계적 특성 향상을 위해서 다양한 종류의 석출물들을 사용한다. 이들 석출물들은 석출 초기에 기지와의 정합성을 유지하기 위해서 준안성 상의 형태로 석출하고, 이 후 다양한 방식으로 안정상으로 변태한다. 철강재료 기지의 상변태는 주로 큰 범위로 일어나서, 일반적인 Macro분석법으로 해석이 용이 하지만, 석출물은 작은 크기로 인하여 EBSD나 SEM등의  분석법으로 해석하기 어렵다. 투과전자현미경은 높은 공간분해능과 결정구조분석 및 화학조성분석이 가능하다는 점에서 이들 석출상의 상변태 거동을 해석하기에 적합하다.

본 발표에서는 철강재료 내부에서 석출하는 다양한 준안정 석출상의 안정상으로의 상변태과정을 투과전자현미경 기법을 통하여 해석한 사례를 제시하고자 한다. 세부적으로는 석출상의 상변태 시 결정구조의 변화와 조성의 변화과정을 조사함 으로써, 무확산변태와 확산변태의 기여를 확인하고자 한다. 최종적으로는 각기 다른 상변태 과정을 선택하는 이유를 준안정상, 안정상, 기지의 조성 및 결정구조 측면에서 생각해 보고자한다.

Keywords: Phase Transformation, Precipitate, steel

[영문초록예시]

Characterization of microstructures and mechanical properties

in diffusion-bonded hot-work tool steels by centrifugal casting

Yoon-Beom Ji1, Hyun Soon Park2

1Sung-Il Turbine, Gangseo-gu

2Department of materials science and engineering, INHA University

E-mail: hsparkinha@inha.ac.kr

In this study, we characterized the microstructures and mechanical properties of diffusion-bonded hot-work tool steels at dual-wall sleeves by centrifugal casting. These characterization techniques provide us with an idea to develop the dual-wall sleeves (inner wall: DIN1.2888, external wall: SCM420H) by centrifugal casting. To understand optimum conditions for manufacturing dual-wall sleeves, we performed preliminary experiments on diffusion bonding properties between molten DIN1.2888 and solid SCM420H can. Changes in elements (Co, W, Fe) and hardness across the regions of DIN1.2888/Diffusion layer/SCM420H have been investigated. We controlled three parameters to influence the diffusion length, i.e., Δt (time gap between molten DIN1.2888 and SCM420H injection: SCM420H maintain temperature), revolutions per minute(rpm), heat treatment(Q/T). Further, a methodology to evaluate the bonding strength of diffusion layer has been proposed.

Keyword: interface, diffusion, microstructures, mechanical properties